*Since 2016/03/31*

1: 2016/03/31~2016/04/13

2: 2016/04/14~2016/04/22

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Fail | | Resolved | | Test |
| Origin | Remain | 1 | 2 | Wan |
| 23 | 23 |  |  | wan\_rfc3315\_rfc3646 |
| 18 | 18 |  |  | wan\_rfc3633 |
| 41 | 41 |  |  | wan\_rfc2460\_rfc4861\_rfc4443 |
| 45 | 45 |  |  | wan\_rfc4862 |
| 14 | 14 |  |  | wan\_rfc1981 |
| 7 | 7 |  |  | wan\_rfc7084 |
|  |  |  |  | Lan |
| 10 |  |  | 10 | lan\_rfc3315 |
| 2 |  |  | 2 | lan\_rfc3736 |
| 1 | 1 |  |  | lan\_rfc2460 |
| 0 |  |  |  | lan\_rfc4861 |
| 21 |  | 21 |  | lan\_rfc4862 |
| 0 |  |  |  | lan\_rfc4443 |
| 13 | 1 | 2 | 10 | lan\_rfc7084 |
|  |  |  |  | Forwarding |
| 19 | 19 |  |  | forward\_rfc2460\_rfc4861\_rfc4443 |
| 2 | 2 |  |  | forward\_rfc7084 |

**20160414**

Resolved

lan7084 test 4

handle\_ipv6.c

Oradvd/radvd.conf

even dhcp6c fail, radvd still need to run

lan7084 test 5

Oradvd/radvd.conf

add route{} option

**20160415**

Resolved

lan3315 test 16

OWideDHCPv6/src/dhcp6s.c

if iana address in dhcp request is different from dhcp advertise, dhcp reply need to add status code notonlink in it iana option

**20160418**

Resolved

lan7084 test6

OWideDHCPv6/src /prefixconf.c

handle\_ipv6.c

lan7084 test7

handle\_ipv6.c

lan3315 test 20

fix by harry

**20160419**

Resolved

lan3315 test 35

same as test 6 dhcp6s.c status code notonlink

lan3315 test29

fix by harry

lan3315 test46

fix by harry

lan3315 test51

fix by harry

lan3315 test25

fix by harry

lan3315 test26

fix by harry

lan3315 test18

fix by harry

lan3736 test14

fix by harry

lan3736 test9

fix by harry

lan7084 test8

handle\_ipv6.c

prefix need a timer

lan7084 test9

prefix need a timer

lan7084 test12

prefix valid time/ preferred time error(same as test 1 2)

**20160420**

Resolved

NO

**20160421**

Resolved

lan7084 test 14

lan7084 test 15

dhcp6c.c

need to implement reconfigure function, when dhcp client receive reconfigure message, it need to send renew message.

lan7084 test 11

update radvd to newer version

**20160422**

Resolved

lan 3315 test 38

dhcp6s.c

declient message will check ip address but wide dhcp6c didn't get the correct address which bind on interface. just comment it out.