*Since 2016/03/31*

1: 2016/03/31~2016/04/13

2: 2016/04/14~2016/04/22

3: 2016/04/25~2016/04/29

4: 2016/05/03~2016/05/06

5: 2016/05/09~2016/05/13

6: 2016/05/16~2016/05/20

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Fail | | Resolved | | | | | | Test |
| Origin | Remain | 1 | 2 | 3 | 4 | 5 | 6 | Wan |
| 23 |  |  |  | 2 | 5 | 4 | 12 | wan\_rfc3315\_rfc3646 |
| 18 |  |  |  | 9 | 4 |  | 5 | wan\_rfc3633 |
| 41 | 38 |  |  |  | 3 |  |  | wan\_rfc2460\_rfc4861\_rfc4443 |
| 26 |  |  |  |  |  |  | 26 | wan\_rfc4862 |
| 14 |  |  |  | 1 | 13 |  |  | wan\_rfc1981 |
| 7 |  |  |  | 5 | 1 |  | 1 | wan\_rfc7084 |
|  |  |  |  |  |  |  |  | Lan |
| 10 |  |  | 10 |  |  |  |  | lan\_rfc3315 |
| 2 |  |  | 2 |  |  |  |  | lan\_rfc3736 |
| 1 | 1 |  |  |  |  |  |  | lan\_rfc2460 |
| 0 |  |  |  |  |  |  |  | lan\_rfc4861 |
| 21 |  | 21 |  |  |  |  |  | lan\_rfc4862 |
| 0 |  |  |  |  |  |  |  | lan\_rfc4443 |
| 13 | 1 | 2 | 10 |  |  |  |  | lan\_rfc7084 |
|  |  |  |  |  |  |  |  | Forwarding |
| 19 | 2 |  |  | 1 | 12 | 3 |  | forward\_rfc2460\_rfc4861\_rfc4443 |
| 2 |  |  |  |  | 2 |  |  | forward\_rfc7084 |

**20160516**

wan 3315 test 41

WideDHCPv6

fix by harry

wan 3315 test 44

WideDHCPv6

fix by harry

wan 7084 test2

no dad ns

fix by manually bind link-local address

wan 4862 test 2 ~ 27

no dad ns

fix by manually bind link-local address

wan 4862 test 28 ~ 46

not yet support (guess previous run by auto-reboot script which cause it fail)

**20160517**

wan 3315 test 28

WideDHCPv6

fix by harry

wan 3315 test 60

WideDHCPv6/ src/addrconf.c

when receive reply dhcp6c try to update address, but since this address already exist, ioctl will return error with message : file exist!, and immediately return

add condition check, if address already exist, don’t call ioctl(), just update timer

**20160518**

wan 3633 test 9

WideDHCPv6

fix by harry

wan 3633 test 11

WideDHCPv6

fix by harry

wan 3633 test 12

WideDHCPv6

fix by harry

wan 3633 test 17

WideDHCPv6

fix by harry

wan 3633 test 18

WideDHCPv6

fix by harry

wan 3315 test 7

WideDHCPv6

add code to do DAD, if fail, send DECLINE MESSAGE

**20160519**

wan 3315 test 24

wan 3315 test 52

wan 3315 test 53

wan 3315 test 54

wan 3315 test 55

wan 3315 test 56

wan 3315 test 73

WideDHCPv6

add code to do DAD, if fail, send DECLINE MESSAGE