*Since 2016/03/31*

1: 2016/03/31~2016/04/13

2: 2016/04/14~2016/04/22

3: 2016/04/25~2016/04/29

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Fail | | Resolved | | | Test |
| Origin | Remain | 1 | 2 | 3 | Wan |
| 23 | 21 |  |  | 2 | wan\_rfc3315\_rfc3646 |
| 18 | 9 |  |  | 9 | wan\_rfc3633 |
| 41 | 41 |  |  |  | wan\_rfc2460\_rfc4861\_rfc4443 |
| 45 | 45 |  |  |  | wan\_rfc4862 |
| 14 | 13 |  |  | 1 | wan\_rfc1981 |
| 7 | 2 |  |  | 5 | wan\_rfc7084 |
|  |  |  |  |  | Lan |
| 10 |  |  | 10 |  | lan\_rfc3315 |
| 2 |  |  | 2 |  | lan\_rfc3736 |
| 1 | 1 |  |  |  | lan\_rfc2460 |
| 0 |  |  |  |  | lan\_rfc4861 |
| 21 |  | 21 |  |  | lan\_rfc4862 |
| 0 |  |  |  |  | lan\_rfc4443 |
| 13 | 1 | 2 | 10 |  | lan\_rfc7084 |
|  |  |  |  |  | Forwarding |
| 19 | 18 |  |  | 1 | forward\_rfc2460\_rfc4861\_rfc4443 |
| 2 | 2 |  |  |  | forward\_rfc7084 |

**20160428**

wan\_rfc7084 test 5

need reconfigure function which has been added in OWideDHCPv6 : 56

wan\_rfc7084 test 6

need reconfigure function which has been added in OWideDHCPv6 : 56

wan\_rfc7084 test 7

need reconfigure function which has been added in OWideDHCPv6 : 56

wan\_rfc7084 test 8

need reconfigure function which has been added in OWideDHCPv6 : 56

wan\_rfc7084 test 9

modify dhcp6c.wide.conf if m-bit set, need request ia-na

wan\_rfc1981 test 7

previous auto-run procedure error

**20160429**

wan 3633 test 3

modify dhcp6c.wide.conf change ia-pd's iaid to 1(non-zero)

wan 3633 test 4

enlarge tester node's timeout to wait ra arrive

wan 3633 test 8

Solicit message format

DUID type:DHCPv6\_DUID\_LLT\_Ether

previous config.pl setting not correct

need to change duid type to llt not default ll

wan 3633 test 28

add a timer to timeout radvd, have added this function for lan 7084, but didn't consider renew/rebind situation

wan 3633 test 29

radvd need a timer to timeout and restart

wan 3633 test 38

add code in dhcp6c.c to check reply for renew message is correct, if not , need resend renew messge

wan 3633 test 39

add code in dhcp6c.c to check reply for rebind message is correct, if not , need resend rebind messge

wan 3633 test 41

radvd timer

wan 3633 test 42

radvd timer

forwarding 2460 test 17

dhcp6c.wide.conf add mbit=1 obit=0 type

wan 3315 test 70

add code in dhcp6c.c to check reply for renew message is correct, if not , need resend renew messge

wan 3315 test 71

add code in dhcp6c.c to check reply for rebind message is correct, if not , need resend rebind messge